Dürmentingen, 19.06.2018

New control unit series Rondex-Juwel® combines maximum functionality with elegant design

With the new comprehensive control unit series Rondex-Juwel® Georg Schlegel GmbH & Co. KG outstandingly merges function and design. This is also confirmed by the Red Dot Award: Product Design 2018, which Schlegel got for its range Rondex-Juwel®.

The modern and extremly flat design of only 2 mm height and the fine surface in the colours anthracite and silver nearly leaves nothing to be desired as to elegance and aesthetic. In case it still has to be a bit more exclusive there is also a particularly appealing stainless steel version available.

Among others, the actuators give a unique and appealing look for example to cockpits of vehicles and yachts, the control panels in lifts or the operating panels of machines. At the same time the Rondex-Juwel® range represents high functionality and quality. The well thought out, robust construction ensures a long lifetime and an optimal handling of many diverse requirements. In addition, the illuminated versions with a good surface illumination are convincing. A further advantage: Rondex-Juwel® is designed for the use in high switching voltages of up to 440 V as well as for very low currents of just a few mA and thus offers a wide range of possible applications.

Optically the actuators harmonise with the proved Rontron-R-Juwel series and thus allow many combination possibilities.

The Rondex-Juwel® actuators are available in umpteen different version and thus are covering nearly every customer requirement. The range comprises for example illuminated and non-illuminated pushbuttons as well as versions with ring illumination. In addition, customer can choose between handy selector switches (illuminated version also available), key switches, buzzers, as well as a WiFi adapter to USB, a WiFi antenna, pilot lights with lenses in different colours and a comprehensive range of accessories. Thanks to the compatibility all USB jacks (USB, RJ-45 etc.) of the Rontron-R-Juwel range can be used. If requested by the customer, it is possible to realise additional inscriptions by using external nameplate holders – the nameplates of the pushbuttons can be exchanged easily from the front. Schlegel also offers suitable contact blocks with screw, push-in and cage-clamp connection and for battery-free wireless technology. The mounting diameter for the Rondex-Juwel® actuators is Ø 22.3 mm, the mounting depth is between 49.5 mm and 68.5 mm (73.5 mm wireless, 74.5 mm AS Interface), depending on the contact block type being used.

Photo

|  |
| --- |
|  |
| The new Rondex-Juwel® actuators fulfill highest requirements as to aesthetic, functionality and flexibility. |

Contact details:

Georg Schlegel GmbH & Co. KG

Wolfgang Zoll

Kapellenweg 4

88525 Dürmentingen

Phone +49 (7371) 502-0

Fax +49 (7371) 502 13

http://www.schlegel.biz

vertrieb@schlegel.biz

Media contact:

Georg Schlegel GmbH & Co. KG

Bernd Geisinger

Kapellenweg 4

88525 Dürmentingen

Phone +49 (7371) 502-0

Fax +49 (7371) 502 49

http://www.schlegel.biz

bernd.geisinger@schlegel.biz

For publication, free of charge. Specimen copy or indication requested.

About Georg Schlegel GmbH & Co. KG

Schlegel stands for innovation, quality and design. Founded in 1945, Schlegel is today a globally operating company with headquarters in Germany, sales offices in Austria and Singapore, and exports to more than 80 countries on all five continents. The core competences: Development and production of control units, pilot lights and terminal blocks. The product portfolio further includes bus systems, enclosures, limit switches, control panels and functional components. When developing new products, Schlegel sets high standards as to the design. More than 90 national and international design awards confirm the company's high level of design expertise, among these prizes are the iF Design Award, the Red Dot Award or the German Design Award.